Package: installation-reports

INSTALL REPORT

Debian-installer-version: 8-24-2004 http://cdimage.debian.org/pub/cdimage-testing/sarge_d-i/i386/rc1/sarge-i386-netinst.iso

uname -a: Linux latitude610 2.4.26-1-386 #1 Thu Jul 22 12:46:23 JST 2004 i686 GNU/Linux

Date: 8-24-2004

Method: How did you install? Boot from CDROM, then network

What did you boot off? CDROM

If network install, from where? Not sure – took the default or first on the list

Proxied? No

Machine: Dell Latitude C610

Processor: Pentium III

Memory: 785 MB

Root Device: IDE-yes SCSI-no Name of device? hda

Root Size/partition table:

Primary partition – Windows FAT32 15 MB

Logical partition - / 14.5 MB

Logical partition – swap 500 MB

Output of lspci

0000:00:00.0 Host bridge: Intel Corp. 82830 830 Chipset Host Bridge (rev 02)

0000:00:01.0 PCI bridge: Intel Corp. 82830 830 Chipset AGP Bridge (rev 02)

0000:00:1d.0 USB Controller: Intel Corp. 82801CA/CAM USB (Hub #1) (rev 01)

0000:00:1e.0 PCI bridge: Intel Corp. 82801 PCI Bridge (rev 41)

0000:00:1f.0 ISA bridge: Intel Corp. 82801CAM ISA Bridge (LPC) (rev 01)

0000:00:1f.1 IDE interface: Intel Corp. 82801CAM IDE U100 (rev 01)

0000:00:1f.5 Multimedia audio controller: Intel Corp. 82801CA/CAM AC'97 Audio Controller (rev 01)

0000:00:1f.6 Modem: Intel Corp. 82801CA/CAM AC'97 Modem Controller (rev 01)

0000:01:00.0 VGA compatible controller: ATI Technologies Inc Radeon Mobility M6 LY

0000:02:00.0 Ethernet controller: 3Com Corporation 3c905C-TX/TX-M [Tornado] (rev 78)

0000:02:01.0 CardBus bridge: Texas Instruments PCI1420

0000:02:01.1 CardBus bridge: Texas Instruments PCI1420

lspci -n:

0000:00:00.0 0600: 8086:3575 (rev 02)

0000:00:01.0 0604: 8086:3576 (rev 02)

0000:00:1d.0 0c03: 8086:2482 (rev 01)

0000:00:1e.0 0604: 8086:2448 (rev 41)

0000:00:1f.0 0601: 8086:248c (rev 01)

0000:00:1f.1 0101: 8086:248a (rev 01)

0000:00:1f.5 0401: 8086:2485 (rev 01)

0000:00:1f.6 0703: 8086:2486 (rev 01)

0000:01:00.0 0300: 1002:4c59

0000:02:00.0 0200: 10b7:9200 (rev 78)

0000:02:01.0 0607: 104c:ac51

0000:02:01.1 0607: 104c:ac51

Base System Installation Checklist:

[O] = OK, [E] = Error (please elaborate below), [ ] = didn't try it

Initial boot worked: [ O]

Configure network HW: [ O]

Config network: [ O]

Detect CD: [ O]

Load installer modules: [ O]

Detect hard drives: [ O]

Partition hard drives: [ O]

Create file systems: [ O]

Mount partitions: [ O]

Install base system: [ O]

Install boot loader: [ O]

Reboot: [ O]

Comments/Problems:

Great installation!! Worked flawlessly! Much better than the stable installation process. I accepted the automatic partition and it worked very well. I installed Windows 2000 on a different partition (before I installed Debian), and the Linux installer added Grub with no problems. I can boot to either partition. I used the default workstation installtion option.

Only one problem. When I tried to print using CUPS, I found that cupsys was not installed. I had to do an apt-get install cupsys to get the server installed and running. After that, I could not log onto the server using the KDE print manger; I had to use the web interface. Once the printers were configured, printing is working.

I also quit the installation process when I got to the email setup options. I did not want to use exim.

Install logs and other status info is available in /var/log/debian-installer/.

Once you have filled out this report, mail it to submit@bugs.debian.org.

2004-08-24T10:01:11