root                                                                                                                                
root
password:                                                                                                                           
xxxxxxx                                                                                                                            
You have new mail in /var/mail/root.
Last login: Fri Jul 25 11:15:17 on ttyS0
lx1sles8:~ #                                                                                                                        
shutdown -r now                                                                                                                     
shutdown -r now
Broadcast message from root (ttyS0) (Fri Jul 25 11:16:10 2003):
The system is going down for reboot NOW!
INIT: Switching to runlevel: 6
lx1sles8:~ #                                                                                                                        
Boot logging started on /dev/ttyS0(/dev/console) at Fri Jul 25 11:16:11 2003
Master Resource Control: previous runlevel: 3, switching to runlevel: 6
Shutting down service at daemon                                                                                                     
..done
Shutting down CRON daemon                                                                                                           
..done
Shutting down Name Service Cache Daemon                                                                                             
..done
Shutting down mail service (Postfix)                                                                                                
..done
Umount SMB File System..unused
Shutting down RPC portmap daemon                                                                                                    
..done
Shutting down SSH daemon..done                                                                                                      
Stopping hotplugging services                                                                                                       
..done
Shutting down syslog servicesJul 25 11:16:12 lx1sles8 kernel: Kernel logging (proc) stopped.
Jul 25 11:16:12 lx1sles8 kernel: Kernel log daemon terminating.
..done
Shutting down network interfaces:
    iucv0                                                                                                                           
..done
    eth1                                                                                                                            
ifdown: Could not get a valid interface name: -> skipped
..done
Saving random seed..done
Running /etc/init.d/halt.local
..doneSending all processes the TERM signal...
 ..done
Sending all processes the KILL signal...h 
md: recovery thread got woken up ...                                                                                                
md: recovery thread finished ...                                                                                                    
md: stopping all md devices.                                                                                                        
01: HCPGSP2629I The virtual machine is placed in CP mode due to a SIGP stop from CPU 01.                                            
00: hwc low level driver: can write messages                                                                                        
00: hwc low level driver: can not read state change notifications                                                                   
00: hwc low level driver: can receive signal quiesce                                                                                
00: hwc low level driver: can read commands                                                                                         
00: hwc low level driver: can read priority commands                                                                                
Linux version 2.4.19-3suse-SMP (root@s390z02) (gcc version 3.2) #1 SMP Wed Nov 6 22:34:43 UTC 2002                                  
We are running under VM (31 bit mode)                                                                                               
This machine has an IEEE fpu                                                                                                        
On node 0 totalpages: 262144                                                                                                        
zone(0): 262144 pages.                                                                                                              
zone(1): 0 pages.                                                                                                                   
zone(2): 0 pages.                                                                                                                   
Building zonelist for node : 0                                                                                                      
Kernel command line: dasd=620-62f root=/dev/dasdm1                                                                                  
Highest subchannel number detected (hex) : 000F                                                                                     
Calibrating delay loop...                                                                                                           
627.50 BogoMIPS                                                                                                                     
Memory: 1032100k/1048576k available (1706k kernel code, 0k reserved, 396k data, 56k init)                                           
Dentry cache hash table entries: 131072 (order: 8, 1048576 bytes)                                                                   
Inode cache hash table entries: 65536 (order: 7, 524288 bytes)                                                                      
Mount-cache hash table entries: 512 (order: 0, 4096 bytes)                                                                          
Buffer-cache hash table entries: 65536 (order: 6, 262144 bytes)                                                                     
Page-cache hash table entries: 262144 (order: 8, 1048576 bytes)                                                                     
debug: Initialization complete                                                                                                      
POSIX conformance testing by UNIFIX                                                                                                 
Detected 2 CPU's                                                                                                                    
Boot cpu address  0                                                                                                                 
cpu 0 phys_idx=0 vers=FF ident=02A07A machine=2066 unused=0000                                                                      
cpu 1 phys_idx=1 vers=FF ident=02A07A machine=2066 unused=0000                                                                      
migration_task 0 on cpu=0                                                                                                           
migration_task 1 on cpu=1                                                                                                           
init_mach : starting machine check handler                                                                                          
Linux NET4.0 for Linux 2.4                                                                                                          
Based upon Swansea University Computer Society NET3.039                                                                             
Initializing RT netlink socket                                                                                                      
mach_handler : ready                                                                                                                
mach_handler : waiting for wakeup                                                                                                   
Starting kswapd                                                                                                                     
kinoded started                                                                                                                     
VFS: Diskquotas version dquot_6.5.0 initialized                                                                                     
aio_setup: num_physpages = 65536                                                                                                    
aio_setup: sizeof(struct page) = 44                                                                                                 
pty: 256 Unix98 ptys configured                                                                                                     
RAMDISK driver initialized: 16 RAM disks of 32768K size 1024 blocksize                                                              
loop: loaded (max 16 devices)                                                                                                       
md: md driver 0.90.0 MAX_MD_DEVS=256, MD_SB_DISKS=27                                                                                
md: Autodetecting RAID arrays.                                                                                                      
md: autorun ...                                                                                                                     
md: ... autorun DONE.                                                                                                               
debug: cio_msg: new level 6                                                                                                         
debug: cio_trace: new level 6                                                                                                       
debug: cio_crw: new level 6                                                                                                         
NET4: Linux TCP/IP 1.0 for NET4.0                                                                                                   
IP Protocols: ICMP, UDP, TCP, IGMP                                                                                                  
IP: routing cache hash table of 4096 buckets, 64Kbytes                                                                              
                                                                                                                                    
TCP: Hash tables configured (established 131072 bind 65536)                                                                         
Linux IP multicast router 0.06 plus PIM-SM                                                                                          
NET4: Unix domain sockets 1.0/SMP for Linux NET4.0.                                                                                 
RAMDISK: Compressed image found at block 0                                                                                          
Freeing initrd memory: 636k freed                                                                                                   
VFS: Mounted root (ext2 filesystem).                                                                                                
Loading module jbd ...                                                                                                              
Using /lib/modules/2.4.19-3suse-SMP/kernel/fs/jbd/jbd.o                                                                             
Journalled Block Device driver loaded                                                                                               
Loading module ext3 ...                                                                                                             
Using /lib/modules/2.4.19-3suse-SMP/kernel/fs/ext3/ext3.o                                                                           
Loading module dasd_mod dasd=$dasd ...                                                                                              
Using /lib/modules/2.4.19-3suse-SMP/kernel/drivers/s390/block/dasd_mod.o                                                            
dasd: initializing...                                                                                                               
debug: dasd: new level 3                                                                                                            
dasd: Registered successfully to major no 94                                                                                        
dasd: initialization finished                                                                                                       
Loading module dasd_eckd_mod ...                                                                                                    
Using /lib/modules/2.4.19-3suse-SMP/kernel/drivers/s390/block/dasd_eckd_mod.o                                                       
dasd(eckd): ECKD discipline initializing                                                                                            
dasd(eckd): /dev/dasdm  ( 94: 48),062c@03: 3390/0A(CU:3990/01) Cyl:3339 Head:15 Sec:224                                             
dasd(eckd): /dev/dasdm  ( 94: 48),062c@03: DIAG210 returned VRDCRCCL = 04, VRDCCRTY = 82, VRDCCRFT = 82                             
dasd(eckd): /dev/dasdm  ( 94: 48),062c@03: XRC_supported reset because of missing VM support                                        
dasd(eckd): /dev/dasdm  ( 94: 48),062c@03: 3390/0A(CU:3990/01): Configuration data read                                             
debug: dasdm: new level 3                                                                                                           
dasd(eckd): /dev/dasdn  ( 94: 52),062d@04: 3390/0A(CU:3990/01) Cyl:3339 Head:15 Sec:224                                             
dasd(eckd): /dev/dasdn  ( 94: 52),062d@04: DIAG210 returned VRDCRCCL = 04, VRDCCRTY = 82, VRDCCRFT = 82                             
dasd(eckd): /dev/dasdn  ( 94: 52),062d@04: XRC_supported reset because of missing VM support                                        
dasd(eckd): /dev/dasdm  ( 94: 48),062c@03: (4kB blks): 2404080kB at 48kB/trk compatible disk layout                                 
dasd(eckd): /dev/dasdn  ( 94: 52),062d@04: 3390/0A(CU:3990/01): Configuration data read                                             
debug: dasdn: new level 3                                                                                                           
dasd(eckd): /dev/dasdo  ( 94: 56),062e@05: 3390/0A(CU:3990/01) Cyl:3339 Head:15 Sec:224                                             
dasd(eckd): /dev/dasdo  ( 94: 56),062e@05: DIAG210 returned VRDCRCCL = 04, VRDCCRTY = 82, VRDCCRFT = 82                             
dasd(eckd): /dev/dasdo  ( 94: 56),062e@05: XRC_supported reset because of missing VM support                                        
dasd(eckd): /dev/dasdn  ( 94: 52),062d@04: (4kB blks): 2404080kB at 48kB/trk compatible disk layout                                 
dasd(eckd): /dev/dasdo  ( 94: 56),062e@05: 3390/0A(CU:3990/01): Configuration data read                                             
debug: dasdo: new level 3                                                                                                           
dasd: waiting for responses...                                                                                                      
dasd(eckd): /dev/dasdo  ( 94: 56),062e@05: (4kB blks): 2404080kB at 48kB/trk compatible disk layout                                 
Partition check:                                                                                                                    
 dasdm:VOL1/  SL862C: dasdm1                                                                                                        
 dasdn:VOL1/  SL862D: dasdn1                                                                                                        
 dasdo:VOL1/  SL862E: dasdo1                                                                                                        
dasd(eckd): We are interested in: CU 3880/00                                                                                        
dasd(eckd): We are interested in: CU 3990/00                                                                                        
dasd(eckd): We are interested in: CU 2105/00                                                                                        
dasd(eckd): We are interested in: CU 9343/00                                                                                        
kjournald starting.  Commit interval 5 seconds                                                                                      
EXT3-fs: mounted filesystem with ordered data mode.                                                                                 
VFS: Mounted root (ext3 filesystem) readonly.                                                                                       
Trying to move old root to /initrd ... no /initrd directory -> okay                                                                 
Unmounting old root                                                                                                                 
Trying to free ramdisk memory ... okay                                                                                              
Freeing unused kernel memory: 14k freed                                                                                             
INIT: version 2.82 booting
Running /etc/init.d/boot
Mounting /proc device..done
Mounting /dev/pts..done
Boot logging started on /dev/ttyS0(/dev/console) at Fri Jul 25 11:16:26 2003
md: Autodetecting RAID arrays.                                                                                                      
md: autorun ...                                                                                                                     
md: ... autorun DONE.                                                                                                               
Run file system check on root for LVM activation
fsck 1.28 (31-Aug-2002)
/dev/dasdm1: clean, 10676/300960 files, 330497/600996 blocks
..doneRemounting root file system (/) read/write for vgscan...
EXT3 FS 2.4-0.9.18, 14 May 2002 on dasd(94,49), internal journal                                                                    
Scanning for LVM volume groups...
LVM version 1.0.5(mp-v6)(15/07/2002) module loaded                                                                                  
vgscan -- reading all physical volumes (this may take a while...)
vgscan -- "/etc/lvmtab" and "/etc/lvmtab.d" successfully created
vgscan -- WARNING: This program does not do a VGDA backup of your volume group
Activating LVM volume groups...
vgchange -- no volume groups found
..done
Activating swap-devices in /etc/fstab...
..doneChecking file systems...
fsck 1.28 (31-Aug-2002)
/dev/dasdm1: clean, 10676/300960 files, 330497/600996 blocks
/dev/dasdo1 has been mounted 28 times without being checked, check forced.
/dev/dasdo1: 13950/300960 files (0.1% non-contiguous), 349156/600996 blocks
/dev/dasdn1: clean, 70797/300960 files, 290037/600996 blocks
..doneEXT3 FS 2.4-0.9.18, 14 May 2002 on dasd(94,49), internal journal                                                              
Mounting local file systems...
proc on /proc type proc (rw)
devpts on /dev/pts type devpts (rw,mode=0620,gid=5)
kjournald starting.  Commit interval 5 seconds                                                                                      
EXT3 FS 2.4-0.9.18, 14 May 2002 on dasd(94,57), internal journal                                                                    
EXT3-fs: mounted filesystem with ordered data mode.                                                                                 
/dev/dasdo1 on /opt type ext3 (rw)
kjournald starting.  Commit interval 5 seconds                                                                                      
EXT3 FS 2.4-0.9.18, 14 May 2002 on dasd(94,53), internal journal                                                                    
EXT3-fs: mounted filesystem with ordered data mode.                                                                                 
/dev/dasdn1 on /usr type ext3 (rw)
mount: going to use the loop device /dev/loop0
/tmp/iso/CD1/7.2-s390-respin-cd1.iso on /mnt/RedHat/CD1 type iso9660 (ro,loop=/dev/loop0)
mount: going to use the loop device /dev/loop1
/tmp/iso/CD1/7.2-s390-respin-cd2.iso: No such file or directory
mount: failed setting up loop device
mount: going to use the loop device /dev/loop2
/tmp/iso/CD1/7.2-s390-respin-cd3.iso: No such file or directory
mount: failed setting up loop device
mount: going to use the loop device /dev/loop3
/tmp/iso/CD4/7.2-s390-respin-cd4.iso on /mnt/RedHat/CD4 type iso9660 (ro,loop=/dev/loop3)
mount: going to use the loop device /dev/loop4
/tmp/iso/CD4/7.2-s390-respin-cd5.iso: No such file or directory
mount: failed setting up loop device
mount: going to use the loop device /dev/loop5
/tmp/iso/CD4/7.2-s390-respin-cd6.iso: No such file or directory
mount: failed setting up loop device
..failedCreating /var/log/boot.msg
..doneRestore device permissions                                                                                                    
..done
Activating remaining swap-devices in /etc/fstab...
..doneMounting shared memory FS on /dev/shm..done
Setting up the system clock..done
Setting up timezone data..done
Setting up hostname 'lx1sles8'..done
Setting up loopback interface                                                                                                       
..done
Enabling syn flood protection..done
Disabling IP forwarding..done
Running /etc/init.d/boot.local
..done                                                                                                                              
INIT: Entering runlevel: 3
Boot logging started on /dev/ttyS0(/dev/console) at Fri Jul 25 11:16:37 2003
Master Resource Control: previous runlevel: N, switching to runlevel: 3
Initializing random number generator..done
Setting up network interfaces:
    lo                                                                                                                              
..done
    eth1                                                                                                                            
IPv6 v0.8 for NET4.0                                                                                                                
IPv6 over IPv4 tunneling driver                                                                                                     
qdio: loading QDIO base support version 2 ($Revision: 1.120.2.1 $/$Revision: 1.56.2.1 $)                                            
debug: qdio_setup: new level 2                                                                                                      
debug: qdio_labs: new level 2                                                                                                       
debug: qdio_sense: new level 2                                                                                                      
debug: qdio_trace: new level 2                                                                                                      
qeth: loading qeth S/390 OSA-Express driver ($Revision: 1.260.2.13 $/$Revision: 1.86.2.2 $/$Revision: 1.31 $:IPv6:VLAN)             
 qeth: allocated 0 spare buffers                                                                                                    
debug: qeth_setup: new level 3                                                                                                      
debug: qeth_misc: new level 2                                                                                                       
debug: qeth_data: new level 2                                                                                                       
debug: qeth_control: new level 2                                                                                                    
debug: qeth_sense: new level 2                                                                                                      
debug: qeth_qerr: new level 2                                                                                                       
debug: qeth_trace: new level 2                                                                                                      
qeth: Trying to use card with devnos 0x100C/0x100D/0x100E                                                                           
 qeth: received an IDX TERMINATE on irq 0x0/0x1 with cause code 0x22 -- try another portname                                        
 qeth: There were problems in hard-setting up the card.                                                                             
qdio: QDIO base support version 2 ($Revision: 1.120.2.1 $/$Revision: 1.56.2.1 $): module removed                                    
ifup: Could not get a valid interface name: -> skipped
..failed
    iucv0                                                                                                                           
IUCV lowlevel driver Version: 1.32.6.6  initialized                                                                                 
iucv0: 'TCPIP'                                                                                                                      
NETIUCV driver Version: 1.17.6.4  initialized                                                                                       
iucv0: connected with remote side                                                                                                   
IP/Peer:        9.89.17.136 / 9.89.17.131  ..done
Starting syslog services..done
Starting hotplugging services  net Ù..done
Starting hardware scan on boot                                                                                                      
..done
Starting RPC portmap daemon..done
Starting SSH daemon                                                                                                                 
..done
Mount SMB File System..unused
Starting mail service (Postfix)                                                                                                     
..done
Starting service at daemon..done                                                                                                    
Starting CRON daemon..done
Starting Name Service Cache Daemon..done
Master Resource Control: runlevel 3 has been reached
_c                                                                                                                                  
Welcome to SuSE SLES 8 (s390) - Kernel 2.4.19-3suse-SMP (ttyS0).
lx1sles8 login:                                                                                                                     
Jul 25 11:16:46 lx1sles8 kernel: klogd 1.4.1, log source = /proc/kmsg started.
Jul 25 11:16:46 lx1sles8 kernel: Inspecting /boot/System.map-2.4.19-3suse-SMP
Jul 25 11:16:46 lx1sles8 kernel: Loaded 9597 symbols from /boot/System.map-2.4.19-3suse-SMP.
Jul 25 11:16:46 lx1sles8 kernel: Symbols match kernel version 2.4.19.
Jul 25 11:16:46 lx1sles8 kernel: Loaded 428 symbols from 10 modules.
Jul 25 11:16:46 lx1sles8 kernel: IPv6 v0.8 for NET4.0
Jul 25 11:16:46 lx1sles8 kernel: IPv6 over IPv4 tunneling driver
Jul 25 11:16:46 lx1sles8 kernel: qdio: loading QDIO base support version 2 ($Revision: 1.120.2.1 $/$Revision: 1.56.2.1 $)
Jul 25 11:16:46 lx1sles8 kernel: debug: qdio_setup: new level 2
Jul 25 11:16:46 lx1sles8 kernel: debug: qdio_labs: new level 2
Jul 25 11:16:46 lx1sles8 kernel: debug: qdio_sense: new level 2
Jul 25 11:16:46 lx1sles8 kernel: debug: qdio_trace: new level 2
Jul 25 11:16:46 lx1sles8 kernel: qeth: loading qeth S/390 OSA-Express driver ($Revision: 1.260.2.13 $/$Revision: 1.86.2.2 $/$Revisio
n: 1.31 $:IPv6:VLAN)
Jul 25 11:16:46 lx1sles8 kernel:  qeth: allocated 0 spare buffers
Jul 25 11:16:46 lx1sles8 kernel: debug: qeth_setup: new level 3
Jul 25 11:16:46 lx1sles8 kernel: debug: qeth_misc: new level 2
Jul 25 11:16:46 lx1sles8 kernel: debug: qeth_data: new level 2
Jul 25 11:16:46 lx1sles8 kernel: debug: qeth_control: new level 2
Jul 25 11:16:46 lx1sles8 kernel: debug: qeth_sense: new level 2
Jul 25 11:16:46 lx1sles8 kernel: debug: qeth_qerr: new level 2
Jul 25 11:16:46 lx1sles8 kernel: debug: qeth_trace: new level 2
Jul 25 11:16:46 lx1sles8 kernel: qeth: Trying to use card with devnos 0x100C/0x100D/0x100E
Jul 25 11:16:46 lx1sles8 kernel:  qeth: received an IDX TERMINATE on irq 0x0/0x1 with cause code 0x22 -- try another portname
Jul 25 11:16:46 lx1sles8 kernel:  qeth: There were problems in hard-setting up the card.
Jul 25 11:16:46 lx1sles8 kernel: qdio: QDIO base support version 2 ($Revision: 1.120.2.1 $/$Revision: 1.56.2.1 $): module removed
Jul 25 11:16:46 lx1sles8 kernel: IUCV lowlevel driver Version: 1.32.6.6  initialized
Jul 25 11:16:46 lx1sles8 kernel: iucv0: 'TCPIP'
Jul 25 11:16:46 lx1sles8 kernel: NETIUCV driver Version: 1.17.6.4  initialized
                                             
Jul 25 11:16:46 lx1sles8 kernel: iucv0: connected with remote side

root                                                                                                                                
root
                                                                                                                               
Password:                                                                                                                           
xxxxxxx                                                                                                                            

You have new mail in /var/mail/root.
                                                                                               
Last login: Fri Jul 25 11:16:03 on ttyS0
                                                                                           
lx1sles8:~ #                                                                                                                        
shutdown -r now                                                                                                                     
shutdown -r now
                                                                                                                    
_

Broadcast message from root (ttyS0) (Fri Jul 25 11:17:03 2003):
The system is going down for reboot NOW!
INIT: Switching to runlevel: 6
lx1sles8:~ #                                                                                                                        
Boot logging started on /dev/ttyS0(/dev/console) at Fri Jul 25 11:17:03 2003
Master Resource Control: previous runlevel: 3, switching to runlevel: 6
Shutting down service at daemon                                                                                                     
..done
Shutting down CRON daemon                                                                                                           
..done
Shutting down Name Service Cache Daemon                                                                                             
..done
Shutting down mail service (Postfix)                                                                                                
..done
Umount SMB File System..unused
Shutting down RPC portmap daemon                                                                                                    
..done
Shutting down SSH daemon..done
Stopping hotplugging services ..done
Shutting down syslog servicesJul 25 11:17:04 lx1sles8 kernel: Kernel logging (proc) stopped.
Jul 25 11:17:04 lx1sles8 kernel: Kernel log daemon terminating.
..done
Shutting down network interfaces:
    iucv0     ..done
    eth1      ifdown: Could not get a valid interface name: -> skipped
..done
Saving random seed..done
Running /etc/init.d/halt.local
..doneSending all processes the TERM signal...
..done
Sending all processes the KILL signal...
md: recovery thread got woken up ...                                                                                                
md: recovery thread finished ...                                                                                                    
md: stopping all md devices.                                                                                                        
01: HCPGSP2629I The virtual machine is placed in CP mode due to a SIGP stop from CPU 01.                                            
00: hwc low level driver: can write messages                                                                                        
00: hwc low level driver: can not read state change notifications                                                                   
00: hwc low level driver: can receive signal quiesce                                                                                
00: hwc low level driver: can read commands                                                                                         
00: hwc low level driver: can read priority commands                                                                                
Linux version 2.4.19-3suse-SMP (root@s390z02) (gcc version 3.2) #1 SMP Wed Nov 6 22:34:43 UTC 2002                                  
We are running under VM (31 bit mode)                                                                                               
This machine has an IEEE fpu                                                                                                        
On node 0 totalpages: 262144                                                                                                        
zone(0): 262144 pages.                                                                                                              
zone(1): 0 pages.                                                                                                                   
zone(2): 0 pages.                                                                                                                   
Building zonelist for node : 0                                                                                                      
Kernel command line: GeneralÙ                                                                                                      
UniqueID=1hQ4.HbKChfRvG13                                                                                                           
HWClass=disk                                                                                                                        
Model=S390 Disk                                                                                                                     
                                                                                                                                    
StatusÙ                                                                                                                            
Configured=yes                                                                                                                      
Available=yes                                                                                                                       
Needed=no                                                                                                                           
                                                                                                                                    
HardwareÙ                                                                                                                          
Bus=0x8b                                                                                                                            
Slot=0x6                                                                                                                            
Function=0x2d                                                                                                                       
BaseClass=0x106                                                                                                                     
DeviceName=S390 Disk                                                                                                                
UnixDevice=/dev/dasdn                                                                                                               
ROMID=062D                                                                                                                          
Res.Size=3,601020,4096                                                                                                              
Res.DiskGeometry=3339,15,12,1                                                                                                       

Highest subchannel number detected (hex) : 000F                                                                                     
Calibrating delay loop...                                                                                                           
629.14 BogoMIPS                                                                                                                     
Memory: 1032100k/1048576k available (1706k kernel code, 0k reserved, 396k data, 56k init)                                           
Dentry cache hash table entries: 131072 (order: 8, 1048576 bytes)                                                                   
Inode cache hash table entries: 65536 (order: 7, 524288 bytes)                                                                      
Mount-cache hash table entries: 512 (order: 0, 4096 bytes)                                                                          
Buffer-cache hash table entries: 65536 (order: 6, 262144 bytes)                                                                     
Page-cache hash table entries: 262144 (order: 8, 1048576 bytes)                                                                     
debug: Initialization complete                                                                                                      
POSIX conformance testing by UNIFIX                                                                                                 
Detected 2 CPU's                                                                                                                    
Boot cpu address  0                                                                                                                 
cpu 0 phys_idx=0 vers=FF ident=02A07A machine=2066 unused=0000                                                                      
cpu 1 phys_idx=1 vers=FF ident=02A07A machine=2066 unused=0000                                                                      
migration_task 0 on cpu=0                                                                                                           
migration_task 1 on cpu=1                                                                                                           
init_mach : starting machine check handler                                                                                          
Linux NET4.0 for Linux 2.4                                                                                                          
Based upon Swansea University Computer Society NET3.039                                                                             
Initializing RT netlink socket                                                                                                      
mach_handler : ready                                                                                                                
mach_handler : waiting for wakeup                                                                                                   
Starting kswapd                                                                                                                     
kinoded started                                                                                                                     
VFS: Diskquotas version dquot_6.5.0 initialized                                                                                     
aio_setup: num_physpages = 65536                                                                                                    
aio_setup: sizeof(struct page) = 44                                                                                                 
pty: 256 Unix98 ptys configured                                                                                                     
RAMDISK driver initialized: 16 RAM disks of 32768K size 1024 blocksize                                                              
loop: loaded (max 16 devices)                                                                                                       
md: md driver 0.90.0 MAX_MD_DEVS=256, MD_SB_DISKS=27                                                                                
md: Autodetecting RAID arrays.                                                                                                      
md: autorun ...                                                                                                                     
md: ... autorun DONE.                                                                                                               
debug: cio_msg: new level 6                                                                                                         
debug: cio_trace: new level 6                                                                                                       
debug: cio_crw: new level 6                                                                                                         
NET4: Linux TCP/IP 1.0 for NET4.0                                                                                                   
IP Protocols: ICMP, UDP, TCP, IGMP                                                                                                  
IP: routing cache hash table of 4096 buckets, 64Kbytes                                                                              
TCP: Hash tables configured (established 131072 bind 65536)                                                                         
Linux IP multicast router 0.06 plus PIM-SM                                                                                          
NET4: Unix domain sockets 1.0/SMP for Linux NET4.0.                                                                                 
RAMDISK: Compressed image found at block 0                                                                                          
Freeing initrd memory: 636k freed                                                                                                   
VFS: Mounted root (ext2 filesystem) readonly.                                                                                       
Freeing unused kernel memory: 14k freed                                                                                             
GeneralÙ: Can't open GeneralÙ                                                                                                     
Kernel panic: Attempted to kill init!                                                                                               
00: HCPGSP2629I The virtual machine is placed in CP mode due to a SIGP stop from CPU 01.                                            
01: HCPGIR450W CP entered; disabled wait PSW 000A0000 80028872                                                                      
00: CLOSE CONSOLE