[Interceptor]
    # This section is for the network traffic interceptor driver.

    # The driver to use:
    driver = user.interceptor
    device_type = acurite-bridge

[[sensor_map]]

        pressure = pressure.00000613.*

  # 5n1
        outTemp = temperature.00008250.*
        outHumidity = humidity.00008250.*
        windSpeed = windspeed.00000613.*
        windDir = winddir.00000613.*
        rain = rainfall.00000613.*
        txBatteryStatus = battery.00000613.*
        rxCheckPercent = rssi.00000613.*

    # Specify the hardware device to capture.  Options include:
    #   acurite-bridge - acurite internet bridge, smarthub, or access
    #   observer - fine offset WH2600/HP1000/HP1003, ambient WS2902
    #   lw30x - oregon scientific LW301/LW302
    #   lacrosse-bridge - lacrosse GW1000U/C84612 internet bridge
    #   wu-client - any hardware that uses the weather underground protocol
    device_type = acurite-bridge