[codec_alaw.so] => (A-law Coder/Decoder)
  == Registered translator 'alawtolin' from format 3 to 6, cost 1
  == Registered translator 'lintoalaw' from format 6 to 3, cost 1
 [codec_a_mu.so] => (A-law and Mulaw direct Coder/Decoder)
  == Registered translator 'alawtoulaw' from format 3 to 2, cost 1
  == Registered translator 'ulawtoalaw' from format 2 to 3, cost 1
 [format_g723.so] => (G.723.1 Simple Timestamp File Format)
  == Registered file format g723sf, extension(s) g723
 [format_wav.so] => (Microsoft WAV format (8000hz Signed Linear))
  == Registered file format wav, extension(s) wav
 [format_mp3.so] => (MPEG-1,2 Layer 3 File Format Support)
  == Registered file format mp3, extension(s) mp3|mpeg3
 [format_wav_gsm.so] => (Microsoft WAV format (Proprietary GSM))
  == Registered file format wav49, extension(s) WAV
 [format_gsm.so] => (Raw GSM data)
  == Registered file format gsm, extension(s) gsm
 [format_vox.so] => (Dialogic VOX (ADPCM) File Format)
  == Registered file format vox, extension(s) vox
 [format_pcm.so] => (Raw uLaw 8khz Audio support (PCM))
  == Registered file format pcm, extension(s) pcm|ulaw|ul|mu
 [format_g729.so] => (Raw G729 data)
  == Registered file format g729, extension(s) g729
 [format_pcm_alaw.so] => (Raw aLaw 8khz PCM Audio support)
  == Registered file format alaw, extension(s) alaw|al
 [format_jpeg.so] => (JPEG (Joint Picture Experts Group) Image Format)
  == Registered format 'jpg' (JPEG (Joint Picture Experts Group))
 [cdr_csv.so] => (Comma Separated Values CDR Backend)
 [cdr_mysql.so] => (MySQL CDR Backend)
  == Parsing '/etc/asterisk/cdr_mysql.conf': Found
 [chan_oh323.so]    -- Got SIP response 481 "Subscription does not exist" back from 217.168.168.49
  == D-Channel on span 1 up
  == Restart on requested on entire span 1
 => (OpenH323 Channel Driver)
  == Parsing '/etc/asterisk/oh323.conf': Found
  0:00.004             OpenH323 Wrapper OpenH323 Wrapper        Version 0.0alpha0 by inAccess Networks (www.inaccessnetworks.com) on Unix Linux (2.4.20-8-i686) at 2003/6/9 16:31:02.846
  == Registered channel type 'OH323' (OpenH323 Channel Driver)
  == OpenH323 Channel Ready (v0.5.2)
 [app_transfer.so] => (Transfer)
  == Registered application 'Transfer'
  == Parsing '/etc/asterisk/enum.conf': Found
Asterisk Ready.
*CLI>     -- B-channel 1 successfully restarted on span 1
    -- B-channel 2 successfully restarted on span 1
    -- B-channel 3 successfully restarted on span 1
    -- B-channel 4 successfully restarted on span 1
    -- B-channel 5 successfully restarted on span 1
    -- B-channel 6 successfully restarted on span 1
    -- B-channel 7 successfully restarted on span 1
    -- B-channel 8 successfully restarted on span 1
    -- B-channel 9 successfully restarted on span 1
    -- B-channel 10 successfully restarted on span 1
    -- B-channel 11 successfully restarted on span 1
    -- B-channel 12 successfully restarted on span 1
    -- B-channel 13 successfully restarted on span 1
    -- B-channel 14 successfully restarted on span 1
    -- B-channel 15 successfully restarted on span 1
    -- B-channel 17 successfully restarted on span 1
    -- B-channel 18 successfully restarted on span 1
    -- B-channel 19 successfully restarted on span 1
    -- B-channel 20 successfully restarted on span 1
    -- B-channel 21 successfully restarted on span 1
    -- B-channel 22 successfully restarted on span 1
    -- B-channel 23 successfully restarted on span 1
    -- B-channel 24 successfully restarted on span 1
    -- B-channel 25 successfully restarted on span 1
    -- B-channel 26 successfully restarted on span 1
    -- B-channel 27 successfully restarted on span 1
    -- B-channel 28 successfully restarted on span 1
    -- B-channel 29 successfully restarted on span 1
    -- B-channel 30 successfully restarted on span 1
    -- B-channel 31 successfully restarted on span 1
WARNING[1167272000]: File chan_zap.c, Line 5275 (pri_fixup): Call specified, but not found?
WARNING[1167272000]: File chan_zap.c, Line 5816 (pri_dchannel): Hangup on bad channel 1
pri debug span 1
Enabled debugging on span 1
< Protocol Discriminator: Q.931 (8)  len=9
< Call Ref: len= 2 (reference 3437/0xD6D) (Originator)
< Message type: RELEASE (77)
< Cause (len= 2) [ Ext: 1  Coding: CCITT (ITU) standard (0) 0: 0   Location: Public network serving the local user (2)
<                  Ext: 1  Cause: Recover on timer expiry (102), class = Protocol Error (6) ]
-- Processing IE 8 (Cause)
> Protocol Discriminator: Q.931 (8)  len=5
> Call Ref: len= 2 (reference 36205/0x8D6D) (Terminator)
> Message type: RELEASE COMPLETE (90)
WARNING[1167272000]: File chan_zap.c, Line 5275 (pri_fixup): Call specified, but not found?
WARNING[1167272000]: File chan_zap.c, Line 5816 (pri_dchannel): Hangup on bad channel 1
< Protocol Discriminator: Q.931 (8)  len=32
< Call Ref: len= 2 (reference 3438/0xD6E) (Originator)
< Message type: SETUP (5)
< Sending Complete (len= 4)
< Bearer Capability (len= 3) [ Ext: 1  Q.931 Std: 0  Info transfer capability: 3.1kHz audio (16)
<                              Ext: 1  Trans mode/rate: 64kbps, circuit-mode (16)
<                              Ext: 1  User information layer 1: A-Law (35)
< Channel ID (len= 5) [ Ext: 1  IntID: Implicit, PRI Spare: 0, Exclusive Dchan: 0
<                        ChanSel: Reserved
<                       Ext: 1  Coding: 0   Number Specified   Channel Type: 3
<                       Ext: 1  Channel: 1 ]
< Progress Indicator (len= 2) [ Ext: 1  Coding: CCITT (ITU) standard (0) 0: 0   Location: Public network serving the local user (2)
<                               Ext: 1  Progress Description: Calling equipment is non-ISDN. (3) ]
< Calling Number (len=12) [ Ext: 0  TON: National Number (2)  NPI: ISDN/Telephony Numbering Plan (E.164/E.163) (1)
<                           Presentation: Unknown (3) '21382890' ]
-- Making new call for cr 3438
-- Processing Q.931 Call Setup
-- Processing IE 33 (Sending Complete)
-- Processing IE 4 (Bearer Capability)
-- Processing IE 24 (Channel Identification)
-- Processing IE 30 (Progress Indicator)
-- Processing IE 108 (Calling Party Number)
> Protocol Discriminator: Q.931 (8)  len=14
> Call Ref: len= 2 (reference 36206/0x8D6E) (Terminator)
> Message type: SETUP ACKNOWLEDGE (13)
> Channel ID (len= 5) [ Ext: 1  IntID: Implicit, PRI Spare: 0, Exclusive Dchan: 0
>                        ChanSel: Reserved
>                       Ext: 1  Coding: 0   Number Specified   Channel Type: 3
>                       Ext: 1  Channel: 1 ]
> Progress Indicator (len= 2) [ Ext: 1  Coding: CCITT (ITU) standard (0) 0: 0   Location: Private network serving the local user (1)
>                               Ext: 1  Progress Description: Called equipment is non-ISDN. (2) ]
< Protocol Discriminator: Q.931 (8)  len=12
< Call Ref: len= 2 (reference 3438/0xD6E) (Originator)
< Message type: STATUS (125)
< Cause (len= 2) [ Ext: 1  Coding: CCITT (ITU) standard (0) 0: 0   Location: Public network serving the local user (2)
<                  Ext: 1  Cause: Protocol error, unspecified (111), class = Protocol Error (6) ]
< Call State (len= 1) [ Ext: 0  Coding: CCITT (ITU) standard (0) Call state: Call Present (6)
-- Processing IE 8 (Cause)
-- Processing IE 20 (Call State)
< Protocol Discriminator: Q.931 (8)  len=32
< Call Ref: len= 2 (reference 3438/0xD6E) (Originator)
< Message type: SETUP (5)
< Sending Complete (len= 4)
< Bearer Capability (len= 3) [ Ext: 1  Q.931 Std: 0  Info transfer capability: 3.1kHz audio (16)
<                              Ext: 1  Trans mode/rate: 64kbps, circuit-mode (16)
<                              Ext: 1  User information layer 1: A-Law (35)
< Channel ID (len= 5) [ Ext: 1  IntID: Implicit, PRI Spare: 0, Exclusive Dchan: 0
<                        ChanSel: Reserved
<                       Ext: 1  Coding: 0   Number Specified   Channel Type: 3
<                       Ext: 1  Channel: 1 ]
< Progress Indicator (len= 2) [ Ext: 1  Coding: CCITT (ITU) standard (0) 0: 0   Location: Public network serving the local user (2)
<                               Ext: 1  Progress Description: Calling equipment is non-ISDN. (3) ]
< Calling Number (len=12) [ Ext: 0  TON: National Number (2)  NPI: ISDN/Telephony Numbering Plan (E.164/E.163) (1)
<                           Presentation: Unknown (3) '21382890' ]
-- Processing Q.931 Call Setup
-- Processing IE 33 (Sending Complete)
-- Processing IE 4 (Bearer Capability)
-- Processing IE 24 (Channel Identification)
-- Processing IE 30 (Progress Indicator)
-- Processing IE 108 (Calling Party Number)
> Protocol Discriminator: Q.931 (8)  len=14
> Call Ref: len= 2 (reference 36206/0x8D6E) (Terminator)
> Message type: SETUP ACKNOWLEDGE (13)
> Channel ID (len= 5) [ Ext: 1  IntID: Implicit, PRI Spare: 0, Exclusive Dchan: 0
>                        ChanSel: Reserved
>                       Ext: 1  Coding: 0   Number Specified   Channel Type: 3
>                       Ext: 1  Channel: 1 ]
> Progress Indicator (len= 2) [ Ext: 1  Coding: CCITT (ITU) standard (0) 0: 0   Location: Private network serving the local user (1)
>                               Ext: 1  Progress Description: Called equipment is non-ISDN. (2) ]
< Protocol Discriminator: Q.931 (8)  len=12
< Call Ref: len= 2 (reference 3438/0xD6E) (Originator)
< Message type: STATUS (125)
< Cause (len= 2) [ Ext: 1  Coding: CCITT (ITU) standard (0) 0: 0   Location: Public network serving the local user (2)
<                  Ext: 1  Cause: Protocol error, unspecified (111), class = Protocol Error (6) ]
< Call State (len= 1) [ Ext: 0  Coding: CCITT (ITU) standard (0) Call state: Call Present (6)
-- Processing IE 8 (Cause)
-- Processing IE 20 (Call State)
< Protocol Discriminator: Q.931 (8)  len=9
< Call Ref: len= 2 (reference 3438/0xD6E) (Originator)
< Message type: DISCONNECT (69)
< Cause (len= 2) [ Ext: 1  Coding: CCITT (ITU) standard (0) 0: 0   Location: Public network serving the local user (2)
<                  Ext: 1  Cause: Recover on timer expiry (102), class = Protocol Error (6) ]
-- Processing IE 8 (Cause)
WARNING[1167272000]: File chan_zap.c, Line 5275 (pri_fixup): Call specified, but not found?
WARNING[1167272000]: File chan_zap.c, Line 5816 (pri_dchannel): Hangup on bad channel 1
< Protocol Discriminator: Q.931 (8)  len=9
< Call Ref: len= 2 (reference 3438/0xD6E) (Originator)
< Message type: RELEASE (77)
< Cause (len= 2) [ Ext: 1  Coding: CCITT (ITU) standard (0) 0: 0   Location: Public network serving the local user (2)
<                  Ext: 1  Cause: Recover on timer expiry (102), class = Protocol Error (6) ]
-- Processing IE 8 (Cause)
> Protocol Discriminator: Q.931 (8)  len=5
> Call Ref: len= 2 (reference 36206/0x8D6E) (Terminator)
> Message type: RELEASE COMPLETE (90)
WARNING[1167272000]: File chan_zap.c, Line 5275 (pri_fixup): Call specified, but not found?
WARNING[1167272000]: File chan_zap.c, Line 5816 (pri_dchannel): Hangup on bad channel 1