Execpt the bugs with UDP sessions, I just discovered that it can't do a plain PAP-login through a modem.
If I check in the /var/log/messages file, I see that the module char-major-108 is missing.
CHAP works fine though...
 
Does anyone know if the UDP problems exists in the RC1 release?
SNF sets improper settings for online games running with udp packets.
 
I tested with another ipchains-script that I've written myself, and shutdown the bastille-firewall, everything works great!
But it would be nice to use the great html-gui (nice work guys) instead of a dumb script.... 
 
AND, it would be nice if you add the ability to use a caching-dns on the LAN-side of the firewall.
I discovered t
 
/joffe
_________________________________________________
TrejComputing AB                     
Jan-Olov Pettersson
 
Besöksadress: Vallhorngatan 20, 124 61 Bandhagen
Adress: Box 87, 124 21 Bandhagen               
Tel: 08-556 294 40, Fax: 08-556 294 41     
Mobil: 0709-73 45 60, P-Fax: 0709-77 83 80