Module: Instantiating suffix
  realm suffix {
        format = "suffix"
        delimiter = "@"
        ignore_default = no
        ignore_null = no
  }
 Module: Linked to module rlm_files
 Module: Instantiating files
  files {
        usersfile = "/etc/freeradius/users"
        acctusersfile = "/etc/freeradius/acct_users"
        preproxy_usersfile = "/etc/freeradius/preproxy_users"
        compat = "no"
  }
 Module: Checking session {...} for more modules to load
 Module: Linked to module rlm_radutmp
 Module: Instantiating radutmp
  radutmp {
        filename = "/var/log/freeradius/radutmp"
        username = "%{User-Name}"
        case_sensitive = yes
        check_with_nas = yes
        perm = 384
        callerid = yes
  }
 Module: Checking post-proxy {...} for more modules to load
 Module: Checking post-auth {...} for more modules to load
 Module: Linked to module rlm_attr_filter
 Module: Instantiating attr_filter.access_reject
  attr_filter attr_filter.access_reject {
        attrsfile = "/etc/freeradius/attrs.access_reject"
        key = "%{User-Name}"
  }
 }
}
server {
 modules {
 Module: Checking authenticate {...} for more modules to load
 Module: Checking authorize {...} for more modules to load
 Module: Linked to module rlm_preprocess
 Module: Instantiating preprocess
  preprocess {
        huntgroups = "/etc/freeradius/huntgroups"
        hints = "/etc/freeradius/hints"
        with_ascend_hack = no
        ascend_channels_per_line = 23
        with_ntdomain_hack = no
        with_specialix_jetstream_hack = no
        with_cisco_vsa_hack = no
        with_alvarion_vsa_hack = no
  }
 Module: Checking preacct {...} for more modules to load
 Module: Checking accounting {...} for more modules to load
 Module: Linked to module rlm_detail
 Module: Instantiating detail
  detail {
        header = "%t"
        detailperm = 384
        dirperm = 493
        locking = no
        log_packet_header = no
  }
 Module: Instantiating attr_filter.accounting_response
  attr_filter attr_filter.accounting_response {
        attrsfile = "/etc/freeradius/attrs.accounting_response"
        key = "%{User-Name}"
  }
 Module: Checking session {...} for more modules to load
 Module: Checking post-proxy {...} for more modules to load
 Module: Checking post-auth {...} for more modules to load
 }
}
radiusd: #### Opening IP addresses and Ports ####
listen {
        type = "auth"
        ipaddr = *
        port = 0
}
listen {
        type = "acct"
        ipaddr = *
        port = 0
}
main {
        snmp = no
        smux_password = ""
        snmp_write_access = no
}
Listening on authentication address * port 1812
Listening on accounting address * port 1813
Listening on proxy address * port 1814
Ready to process requests.
rad_recv: Accounting-Request packet from host 192.168.2.50 port 32768, id=40, le                                                             ngth=202
        User-Name = "irech"
        NAS-Port = 1
        NAS-IP-Address = 192.168.2.50
        Framed-IP-Address = 192.168.20.12
        NAS-Identifier = "C4402-VDI1-3-1"
        Airespace-Wlan-Id = 1
        Acct-Session-Id = "4c44422c/00:12:f0:e1:cc:47/9"
        Acct-Authentic = Remote
        Tunnel-Type:0 = VLAN
        Tunnel-Medium-Type:0 = IEEE-802
        Tunnel-Private-Group-Id:0 = "20"
        Acct-Status-Type = Stop
        Acct-Input-Octets = 344671
        Acct-Output-Octets = 442223
        Acct-Input-Packets = 9426
        Acct-Output-Packets = 749
        Acct-Terminate-Cause = User-Request
        Acct-Session-Time = 356
        Acct-Delay-Time = 0
        Calling-Station-Id = "192.168.20.12"
        Called-Station-Id = "192.168.2.50"
+- entering group preacct
++[preprocess] returns ok
    rlm_realm: No '@' in User-Name = "irech", looking up realm NULL
    rlm_realm: No such realm "NULL"
++[suffix] returns noop
++[files] returns noop
+- entering group accounting
rlm_detail: (null) expands to È¼ÿ¿?¼ÿ¿ddR·?»ÿ¿????pÝÿ¿È¼ÿ¿
        expand: %t -> Mon Jul 19 14:22:35 2010
++[detail] returns ok
++[unix] returns ok
        expand: /var/log/freeradius/radutmp -> /var/log/freeradius/radutmp
        expand: %{User-Name} -> irech
rlm_radutmp: Logout for NAS C4402-VDI1-3-1 port 1, but no Login record
++[radutmp] returns ok
        expand: %{User-Name} -> irech
 attr_filter: Matched entry DEFAULT at line 12
++[attr_filter.accounting_response] returns updated
Sending Accounting-Response of id 40 to 192.168.2.50 port 32768
Finished request 0.
Cleaning up request 0 ID 40 with timestamp +56
Going to the next request
Ready to process requests.
rad_recv: Access-Request packet from host 192.168.2.50 port 32768, id=7, length=                                                             138
        User-Name = "irech"
        User-Password = "tmcqtv0"
        Service-Type = Login-User
        NAS-IP-Address = 192.168.2.50
        NAS-Identifier = "C4402-VDI1-3-1"
        NAS-Port-Type = Wireless-802.11
        Airespace-Wlan-Id = 1
        Calling-Station-Id = "192.168.20.12"
        Called-Station-Id = "192.168.2.50"
        Message-Authenticator = 0xcc6f35b0c7c5257fe37e64741b0d5190
+- entering group authorize
++[preprocess] returns ok
++[chap] returns noop
++[mschap] returns noop
    rlm_realm: No '@' in User-Name = "irech", looking up realm NULL
    rlm_realm: No such realm "NULL"
++[suffix] returns noop
  rlm_eap: No EAP-Message, not doing EAP
++[eap] returns noop
++[unix] returns notfound
++[files] returns noop
++[expiration] returns noop
++[logintime] returns noop
rlm_pap: WARNING! No "known good" password found for the user.  Authentication m                                                             ay fail because of this.
++[pap] returns noop
auth: No authenticate method (Auth-Type) configuration found for the request: Re                                                             jecting the user
auth: Failed to validate the user.
Login incorrect: [irech/tmcqtv0] (from client C4402-VDI1-3-1 port 0 cli 192.168.                                                             20.12)
  Found Post-Auth-Type Reject
+- entering group REJECT
        expand: %{User-Name} -> irech
 attr_filter: Matched entry DEFAULT at line 11
++[attr_filter.access_reject] returns updated
Delaying reject of request 1 for 1 seconds
Going to the next request
Waking up in 0.9 seconds.
Sending delayed reject for request 1
Sending Access-Reject of id 7 to 192.168.2.50 port 32768
Waking up in 4.9 seconds.
Cleaning up request 1 ID 7 with timestamp +135
Ready to process requests.
rad_recv: Access-Request packet from host 127.0.0.1 port 41952, id=44, length=57
        User-Name = "irech"
        User-Password = "tmcqtv0"
        NAS-IP-Address = 192.168.55.150
        NAS-Port = 10
+- entering group authorize
++[preprocess] returns ok
++[chap] returns noop
++[mschap] returns noop
    rlm_realm: No '@' in User-Name = "irech", looking up realm NULL
    rlm_realm: No such realm "NULL"
++[suffix] returns noop
  rlm_eap: No EAP-Message, not doing EAP
++[eap] returns noop
++[unix] returns notfound
++[files] returns noop
++[expiration] returns noop
++[logintime] returns noop
rlm_pap: WARNING! No "known good" password found for the user.  Authentication m                                                             ay fail because of this.
++[pap] returns noop
auth: No authenticate method (Auth-Type) configuration found for the request: Re                                                             jecting the user
auth: Failed to validate the user.
Login incorrect: [irech/tmcqtv0] (from client localhost port 10)
  Found Post-Auth-Type Reject
+- entering group REJECT
        expand: %{User-Name} -> irech
 attr_filter: Matched entry DEFAULT at line 11
++[attr_filter.access_reject] returns updated
Delaying reject of request 2 for 1 seconds
Going to the next request
Waking up in 0.9 seconds.
Sending delayed reject for request 2
Sending Access-Reject of id 44 to 127.0.0.1 port 41952
Waking up in 4.9 seconds.
Cleaning up request 2 ID 44 with timestamp +914
Ready to process requests.